USB to RS485 Converter

Driver Installation

The drivers are located on the CD on the following path

## X:\ usb_485_converter\driver

At the first connection of the device to USB cable the follow window will appear.

Select “install from specific location” and then clicking “NEXT” button the window bellow appears:

Select the path of the local directory containing the drivers

X:\ usb_485_converter\driver
and click “NEXT”.
If the path is correct the follow window will appear, otherwise read wrong installation section of this manual

Click “FINISH” and Windows will install the converter.

NOTE: WIN98 require about 15 second to recognize the converter.

The driver installed work correctly with WinXP, but it isn’t XP certified version then the follow window will appear

You have to click “continue anyway” and install another time the driver.

To check the correct installation and COM assigned to converter open the control panel from start menu, select system and then device manager. The follow window will appear:

To change serial port click on the USB Serial Port (COM3), Port Setting, Advanced and the follow window will appear:

Select the COM number preferred from 1 to 256 and click OK. WARNING: not select a COM number already present.

# UNINSTALLATION

To uninstall the driver you have to click installation application from control pannel and select “USB to serial converter driver” disconnect the converter from PC, click on the remove button and the driver will be removed.

# WRONG INSTALLATION

If the system doesn’t install the device correctly may be wrong driver selection was done. Select device manager from system menu and the next window will appear:

Click on “USB serial port” and remove the device then disconnect the converter from PC and make a new installation.