1000:"Fill in air flow rate."
1001:"Fill in air temperature in."
1002:"Fill in water temperature in."
1003:"Fill in desired capacity"
1004:"Fill in condensation temperature."
1005:"Fill in evaporation temperature."
1009:"Do not state both air temp out and capacity."
1010:"Do not state both water temp out and capacity."
1011:"Enter air humidity."
1012:"Air temp out must be less than air temp in."
1013:"Air temp out must be greater than water temp in."
1014:"Water temp out must be greater than water temp in."
1015:"Water temp out must be less than air temp in."
1016:"Air temp out must be greater than air temp in."
1017:"Air temp out must be less than water temp in."
1018:"Water temperature out must be less than water temperature in."
1019:"Water temperature out must be greater than air temperature in."
1020:"Ethylen glycol content must not be greater than 60%."
1021:"Propylen glycol content must be between10% and 50%."
1022:"Ethanol content must be between10% and 45%."
1023:"Calcium chloride content must not be greater than 30%."
1024:"Potassium carbonate content must be 28% or 37%."
1025:"water flow rate must be between 0.01 and100 kg/s."
1027:"air flow rate must be between 0.02 and 50 kg/s."
1030:"Invalid humidity."
1033:"Air flow rate is too small."
1034:"Air flow rate is too large."
1035:"Evaporation temperature must be less than air temperature."
1036:"Condensation temperature must be greater than air temperature."
1040:"Do not fill in both water flow rate and water temperature out."
1045:"Non-existing coil type"
1048:"Invalid material code"
1056:"Invalid water connection"
1057:"Invalid circuitry"
1058:"Invalid fin pitch"
1059:"Invalid number of tube rows"
1060:"Invalid length"
1061:"Invalid width (height)"
1062:"Do not state both external and finned length"
1063:"Do not state both external and finned width (height)"
1066:"This medium does not exist - select from the list."
1072:"Laminar flow. "
1075:"Air pressure drop greater than maximum. "
1076:"Water pressure drop greater than maximum. "
1077:"The desired capacity will not be reached. "
1078:"The capacity will be greater than desired. "
1081:""Too large a-measure"  (even external dimension)"
1082:"Too large b-measure"  (even external dimension)
1084:"Too high temperature"
1098:"Invalid content of Tyfoxit"
1099:"Freezium content should be19-50%"
2004:"Refrigerant pressure drop greater then maximum. "
2005:"Ready-to-use mixture, do not enter percentage."
2006:"The Pekasol content must not be less then 50%."
2059:"HYCOOL is ready-to-use mixture, do not enter percentage."
2060:"Biotherm content must be between 70% and 40%."
2076:"Too low temperature"
2077:"Invalid input"
2084:"Invalid antifreeze content"
2093:"Built-in headers are recommended at duct pressure greater than 300 Pa"
2094:"Too narrow fin pitch when risk for condensate at air temp below10 deg C"
2095:"Invalid code for installation alternative"
2096:"State either pole number or sound demands" (Air blast coolers)
2097:"First state size and capacity variant"
2098:"Steam connection is too small"
2099:"Condensate connection is too small"
2100:"Check air settings"
2101:"Check water settings"
2102:"Check general settings"
2103:"Steel headers should be used with this header size"
2104:"Input water flow rate was ignored, because of laminar flow..."
2105:"Input water flow rate was ignored, because of too high water flow rate..."