[227-024-05]
Controll=ON/OFF + Tri-state
Voltage= 24 VAC (50/60 Hz) / DC ±20%
Torque=5Nm
[227-024-08]
Controll=ON/OFF + Tri-state
Voltage= 24 VAC (50/60 Hz) / DC ±20%
Torque=8Nm
[227-024-08]
Controll=ON/OFF + Tri-state
Voltage= 24 VAC (50/60 Hz) / DC ±20%
Torque=15Nm
[SM24A-TP]
Controll=ON/OFF + Tri-state
Voltage= 24 VAC (50/60 Hz) / DC ±20%
Torque=20Nm
[227-230-05]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ±15%
Torque=5Nm
[227-230-08]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ±15%
Torque=8Nm
[232D2-230-15]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ±15%
Torque=15Nm
[SM230A-TP]
Controll=Open-close or 3-point
Voltage=100 ... 240 V, 50/60 Hz
Torque=20Nm
[GM230A-TP]
Controll=Open-close
Voltage=100 ... 240 V, 50/60 Hz
Torque=40Nm
[227C-024-05]
Controll= 0...10 VDC
Voltage=24 VAC (50/60 Hz) / DC ±20%
Torque=5Nm
[227C-024-08]
Controll= 0...10 VDC
Voltage=24 VAC (50/60 Hz) / DC ±20%
Torque=8Nm
[232C-024-15]
Controll= 0...10 VDC
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=15Nm
[GM24A-SR-TP]
Controll=Modulating DC 0-10 V
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=20Nm
[GM24A-SR-TP]
Controll=Modulating DC 0-10 V
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=40Nm
[SM24A-SR-TP]
Controll=DC 0 ... 10 V
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=20Nm
[LM230A-TP]
Controll=ON/OFF
Voltage=AC 100 ... 240 V, 50/60 Hz
Torque=5Nm
[LM24A-TP]
Controll=ON/OFF
Voltage=AC 24 V, 50/60 Hz, DC 24 V
Torque=5Nm
[LM230A-SR-TP]
Controll=0-10 V DC
Voltage=AC 100 ... 240 V, 50/60 Hz
Torque=5Nm
[NM24A-TP]
Controll=ON/OFF or 3-point
Voltage=AC 24 V, 50/60 Hz
Torque=10Nm
[NM230A-TP]
Controll=ON/OFF or 3-point
Voltage=AC 100 ... 240 V, 50/60 Hz
Torque=10Nm
[NM24A-SR-TP]
Controll=0-10 V DC
Voltage=AC 24 V, 50/60 Hz
Torque=10Nm
[NF230A]
Spring=YES
Controll=ON/OFF
Voltage=AC 230 V, 50/60 Hz
TorqueDrive=10Nm
TorgueSpring=10Nm
[NF24A]
Spring=YES
Controll=ON/OFF
Voltage=AC 24 V, 50/60 Hz / DC 24 V
TorqueDrive=10Nm
TorgueSpring=10Nm
[SF24A]
Spring=YES
Controll=ON/OFF
Voltage=AC 24 V, 50/60 Hz / DC 24 V
TorqueDrive=20Nm
TorgueSpring=20Nm
[SF230A]
Spring=YES
Controll=ON/OFF
Voltage=AC 230 V, 50/60 Hz
TorqueDrive=20Nm
TorgueSpring=20Nm
[SF24A-SR]
Spring=YES
Controll=0-10 V DC
Voltage=AC 24 V, 50/60 Hz / DC 24 V
TorqueDrive=20Nm
TorgueSpring=20Nm
[SM230A-TP]
Controll=ON/OFF or 3-point
Voltage=AC 100 ... 240 V, 50/60 Hz
Torque=20Nm
[SM24A-TP]
Controll=ON/OFF or 3-point
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=20Nm
[SM24A-SR-TP]
Controll=0-10 V DC
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=20Nm