[SF24A-SR]
Spring=YES
Controll=0-10 V DC
Voltage=AC 24V (50/60 Hz) / DC 24V
Torque=20Nm
[238C-024-15]
Spring=YES
Controll=0-10 V DC
Voltage=24 VAC (50/60 Hz) / DC ±20%
Torque=15Nm
[SF230A]
Spring=true
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz)
Torque=20Nm
[227S-230-05]
Controll=2 point ON/OFF
Voltage=24 VAC (50/60 HZ) / DC ±20%
Torque=5Nm
[341-230-05]
Spring=true
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
TorqueDrive=4Nm
TorgueSpring=5Nm
[238-230-15]
Spring=true
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=15Nm
[238-230-15]
Spring=true
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=15Nm
[Request]
Spring=true
Controll=ON/OFF
Voltage=230 VAC
[227-230-05]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ±15%
Torque=5Nm
[227-230-08]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=8Nm
[232D2-230-15]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=15Nm
[GM230A-TP]
Controll=Open-close
Voltage=AC  100 ... 240 V, 50/60 Hz
Torque=40Nm
[SM230A-TP]
Controll=Open-close or 3-point
Voltage=AC  100 ... 240 V, 50/60 Hz
Torque=20Nm
[227-230-05]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=5Nm
[227-230-08]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=8Nm
[232D2-230-15]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=15Nm
[SM230A-TP]
Controll=Open-close or 3-point
Voltage=AC  100 ... 240 V, 50/60 Hz
Torque=20Nm
[GM230A-TP]
Controll=Open-close 
Voltage=AC  100 ... 240 V, 50/60 Hz
Torque=40Nm
[Request]
Controll=ON/OFF
Voltage=230 VAC
[SF24A-SR]
Spring=YES
Controll=0-10 V DC
Voltage=AC 24V (50/60 Hz) / DC 24V
Torque=20Nm
[238C-024-15]
Spring=YES
Controll=0-10V
Voltage=24 VAC (50/60 Hz) / DC ±20%
Torque=15Nm
[Request]
Spring=YES
Controll=0-10 V DC
Voltage=24 VAC (50/60 Hz) / DC ±20%
[227C-024-05]
Controll=0-10 VDC
Voltage=24 VAC (50/60 Hz) / DC ±20%
Torque=5Nm
[227C-024-08]
Controll=0-10 VDC
Voltage=24 VAC (50/60 Hz) / DC ±20%
Torque=8Nm
[232C-024-15]
Controll=ON/OFF
Voltage=230 VAC (50/60 Hz) ± 15%
Torque=15Nm
[SM24A-SR-TP]
Controll=Modulating DC 0-10 V
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=20Nm
[GM24A-SR-TP]
Controll=Modulating DC 0-10 V
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=40Nm
[...................................naujos pavaros]
[LM230A-TP]
Controll=ON/OFF
Voltage=AC 100 ... 240 V, 50/60 Hz
Torque=5Nm
[LM24A-TP]
Controll=ON/OFF
Voltage=AC 24 V, 50/60 Hz, DC 24 V
Torque=5Nm
[LM230A-SR-TP]
Controll=0-10 V DC
Voltage=AC 100 ... 240 V, 50/60 Hz
Torque=5Nm
[NM24A-TP]
Controll=ON/OFF or 3-point
Voltage=AC 24 V, 50/60 Hz
Torque=10Nm
[NM230A-TP]
Controll=ON/OFF or 3-point
Voltage=AC 100 ... 240 V, 50/60 Hz
Torque=10Nm
[NM24A-SR-TP]
Controll=0-10 V DC
Voltage=AC 24 V, 50/60 Hz
Torque=10Nm
[NF230A]
Spring=YES
Controll=ON/OFF
Voltage=AC 230 V, 50/60 Hz
TorqueDrive=10Nm
TorgueSpring=10Nm
[NF24A]
Spring=YES
Controll=ON/OFF
Voltage=AC 24 V, 50/60 Hz / DC 24 V
TorqueDrive=10Nm
TorgueSpring=10Nm
[SF24A]
Spring=YES
Controll=ON/OFF
Voltage=AC 24 V, 50/60 Hz / DC 24 V
TorqueDrive=20Nm
TorgueSpring=20Nm
[SF230A]
Spring=YES
Controll=ON/OFF
Voltage=AC 230 V, 50/60 Hz
TorqueDrive=20Nm
TorgueSpring=20Nm
[SF24A-SR]
Spring=YES
Controll=0-10 V DC
Voltage=AC 24 V, 50/60 Hz / DC 24 V
TorqueDrive=20Nm
TorgueSpring=20Nm
[SM230A-TP]
Controll=ON/OFF or 3-point
Voltage=AC 100 ... 240 V, 50/60 Hz
Torque=20Nm
[SM24A-TP]
Controll=ON/OFF or 3-point
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=20Nm
[SM24A-SR-TP]
Controll=0-10 V DC
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=20Nm
[LM24A-SR]
Controll=0-10 V DC
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=5Nm
[LM24A-SR-TP]
Controll=0-10 V DC
Voltage=AC 24 V, 50/60 Hz / DC 24 V
Torque=5Nm
[...................................EX pavaros]
[EXNM0G1230S000]
INFO=Quarter turn actuator, ATEX, 10 Nm,  Star 12 , 230 V, ON OFF 3 P
[EXNM0B1230S000]
INFO=Quarter turn actuator, ATEX, 10 Nm,  Star 12 , 24 V, ON OFF 3 P
[EXNR0BSR10L000]
INFO=Quarter turn actuator, ATEX, 10 Nm,  Star 12 , 24 V, Modulating
[EXBG0A0012U000]
Spring=YES
INFO=180°  turn actuator, ATEX, 11 Nm,  Star 12 , 230 V, ON OFF + Spring return
[EXBG0B0012R000]
Spring=YES
INFO=180°  turn actuator, ATEX, 11 Nm,  Star 12 , 24 V, ON OFF + Spring return
[EXAF0B0010U000]
Spring=YES
INFO=Quarter turn actuator, ATEX, 20 Nm,  Star 12 , 24 V, ON OFF + Spring return
[EXAF0A0010U000]
Spring=YES
INFO=Quarter turn actuator, ATEX, 20 Nm,  Star 12 , 230 V, ON OFF + Spring return
[EXAF0BMF10U000]
Spring=YES
INFO=Quarter turn actuator, ATEX, 20 Nm,  Star 12 , 24 V, Modulating 0..10 Vcc + spring return
[EXSM0G1230R000]
INFO=Quarter turn actuator, ATEX, 20 Nm,  Star 12 , 230 V, ON OFF 3 P
[EXSM0B1230R000]
INFO=Quarter turn actuator, ATEX, 20 Nm,  Star 12 , 24 V, ON OFF 3 P
[EXSM0BMF10R000]
INFO=Quarter turn actuator, ATEX, 20 Nm,  Star 12 , 24 V, Modulating
[EXNMOBSR20S000]
INFO=Quarter turn actuator, ATEX, 10 Nm,  Star 12 , 24 V
[EXAMGG1230R000]
INFO=Quarter turn actuator, ATEX, 40 Nm,  Star 12 , 230 V, ON OFF 3 P
[EXAMGB1230R000]
INFO=Quarter turn actuator, ATEX, 40 Nm,  Star 12 , 24 V, ON OFF 3 P
[EXAMGBMF20R000]
INFO=Quarter turn actuator, ATEX, 40 Nm,  Star 12 , 24 V, Modulating
[EXAFOA0010U000]
Spring=YES
INFO=Quarter turn actuator, ATEX, 15 Nm,  Star 12 , 230 V, ON OFF + Spring return
[EXAFOB0010U000]
Spring=YES
INFO=Quarter turn actuator, ATEX, 15 Nm,  Star 12 , 24 V, ON OFF + Spring return
[EXAFOBMF20U000]
Spring=YES
INFO=Quarter turn actuator, ATEX, 15 Nm,  Star 12 , 24 V, Modulating 0..10 Vcc + spring return
[EXAF0BMF10R000]
Spring=YES
INFO=Quarter turn actuator, ATEX, 20 Nm,  Star 12 , 24 V, Modulating 0..10 Vcc + spring return
